1. Please read instruction doc from Readme.pdf which under folder flash\_download\_tool\_v3.8.5
2. Suggest to download the WIFI code before flash the STM32 Application/bootloader code, this is because STM32 application code will configure EPS32 WROOM module enable pin to false.
3. Using flash\_download\_tool\_3.8.5.exe tools to flash the code WIFI ESP32 WROOM module, select firmware factory\_WROOM-32\_AT\_UART0\_version2.bin
4. Require USB to UART device to flash the code
5. Configure the setting show in below

